# 
#
# For more info:
# https://github.com/arduino/Arduino/wiki/Arduino-IDE-1.5---3rd-party-Hardware-specification

name=STM32F4 Boards (STM32duino.com)
version=0.1.0

# compiler variables
# ----------------------
compiler.path={runtime.tools.arm-none-eabi-gcc.path}/bin/
compiler.c.cmd=arm-none-eabi-gcc
compiler.c.flags=-c -g {build.flags.optimize} -Wall -MMD -std=gnu11 -ffunction-sections -fdata-sections -nostdlib --param max-inline-insns-single=500 -DBOARD_{build.variant} {build.vect_flags} -DERROR_LED_PORT={build.error_led_port} -DERROR_LED_PIN={build.error_led_pin}
compiler.c.elf.cmd=arm-none-eabi-g++
compiler.c.elf.flags={build.flags.optimize} -Wl,--gc-sections {build.flags.ldspecs}
compiler.S.cmd=arm-none-eabi-gcc
compiler.S.flags=-c -g -x assembler-with-cpp -MMD
compiler.cpp.cmd=arm-none-eabi-g++
compiler.cpp.flags=-c -g {build.flags.optimize} -Wall -MMD -std=gnu++11 -ffunction-sections -fdata-sections -nostdlib --param max-inline-insns-single=500 -fno-rtti -fno-exceptions -DBOARD_{build.variant} {build.vect_flags} -DERROR_LED_PORT={build.error_led_port} -DERROR_LED_PIN={build.error_led_pin}
compiler.ar.cmd=arm-none-eabi-ar
compiler.ar.flags=rcs
compiler.objcopy.cmd=arm-none-eabi-objcopy
compiler.objcopy.eep.flags=-O ihex -j .eeprom --set-section-flags=.eeprom=alloc,load --no-change-warnings --change-section-lma .eeprom=0
compiler.elf2hex.flags=-O binary
compiler.elf2hex.cmd=arm-none-eabi-objcopy
compiler.ldflags={build.flags.ldspecs}
compiler.size.cmd=arm-none-eabi-size
compiler.define=-DARDUINO=                            

# this can be overriden in boards.txt
build.f_cpu=168000000L
build.mcu=cortex-m4
build.cpu_flags=
build.hs_flag=
build.common_flags=-mthumb -D__STM32F4__
build.extra_flags= {build.cpu_flags} {build.hs_flag} {build.common_flags}
build.flags.optimize=-Os
build.flags.ldspecs=

# These can be overridden in platform.local.txt
compiler.c.extra_flags=
compiler.c.elf.extra_flags="-L{build.variant.path}/ld"
compiler.cpp.extra_flags= 
compiler.S.extra_flags=
compiler.ar.extra_flags=
compiler.elf2hex.extra_flags=


##compiler.libs.c.flags="-I{build.system.path}/libmaple" "-I{build.system.path}/libmaple/include" "-I{build.system.path}/libmaple/stm32f1/include"                                                           "-I{build.system.path}/libmaple/usb/stm32f1" "-I{build.system.path}/libmaple/usb/usb_lib" 
#compiler.libs.c.flags="-I{build.core.path}" "-I{build.core.path}/libmaple" "-I{build.core.path}/libmaple/usbF4" "-I{build.core.path}/libmaple/usbF4/STM32_USB_Device_Library/Core/inc" "-I{build.core.path}/libmaple/usbF4/STM32_USB_Device_Library/Class/cdc/inc" "-I{build.core.path}/libmaple/usbF4/STM32_USB_OTG_Driver/inc" "-I{build.core.path}/libmaple/usbF4/VCP" 
compiler.libs.c.flags="-I{build.system.path}/libmaple" "-I{build.core.path}/libmaple/usbF4"




# USB Flags
# ---------
## build.usb_flags=-DUSB_VID={build.vid} -DUSB_PID={build.pid} -DUSBCON '-DUSB_MANUFACTURER={build.usb_manufacturer}' '-DUSB_PRODUCT={build.usb_product}'

# Default usb manufacturer will be replaced at compile time using
# numeric vendor ID if available or by board's specific value. 
## build.usb_manufacturer="Unknown"


# build patterns
# ---------------------

## Compile c files
recipe.c.o.pattern="{compiler.path}{compiler.c.cmd}" {compiler.c.flags} -mcpu={build.mcu} -DF_CPU={build.f_cpu} -DARDUINO={runtime.ide.version} -DARDUINO_{build.board} -DARDUINO_ARCH_{build.arch} {compiler.c.extra_flags} {build.extra_flags} {build.cpu_flags} {build.vect_flags} {compiler.libs.c.flags} {includes} "{source_file}" -o "{object_file}"

## Compile c++ files
recipe.cpp.o.pattern="{compiler.path}{compiler.cpp.cmd}" {compiler.cpp.flags} -mcpu={build.mcu} -DF_CPU={build.f_cpu} -DARDUINO={runtime.ide.version} -DARDUINO_{build.board} -DARDUINO_ARCH_{build.arch} {compiler.cpp.extra_flags} {build.extra_flags} {build.cpu_flags} {build.vect_flags} {build.hs_flag} {build.common_flags} {compiler.libs.c.flags} {includes} "{source_file}" -o "{object_file}"

## Compile S files
recipe.S.o.pattern="{compiler.path}{compiler.c.cmd}" {compiler.S.flags} -mcpu={build.mcu} -DF_CPU={build.f_cpu} -DARDUINO={runtime.ide.version} -DARDUINO_{build.board} -DARDUINO_ARCH_{build.arch} {compiler.S.extra_flags} {build.extra_flags} {build.cpu_flags} {build.vect_flags} {build.hs_flag} {build.common_flags} {compiler.libs.c.flags} {includes} "{source_file}" -o "{object_file}"

## Create archives
recipe.ar.pattern="{compiler.path}{compiler.ar.cmd}" {compiler.ar.flags} {compiler.ar.extra_flags} "{archive_file_path}" "{object_file}"

## Combine gc-sections, archives, and objects
##recipe.c.combine.pattern="{compiler.path}{compiler.c.elf.cmd}" {compiler.c.elf.flags} -mcpu={build.mcu} "-T{build.variant.path}/{build.ldscript}" "-Wl,-Map,{build.path}/{build.project_name}.map" {compiler.c.elf.extra_flags} -o "{build.path}/{build.project_name}.elf" "-L{build.path}" -lm -lgcc -mthumb -Wl,--cref -Wl,--check-sections -Wl,--gc-sections -Wl,--entry=Reset_Handler -Wl,--unresolved-symbols=report-all -Wl,--warn-common -Wl,--warn-section-align -Wl,--warn-unresolved-symbols -Wl,--start-group "{build.path}/syscalls_sam3.c.o" {object_files} "{build.variant.path}/{build.variant_system_lib}" "{archive_file_path}" -Wl,--end-group
#-Wl,--entry=__start__ 
#recipe.c.combine.pattern="{compiler.path}{compiler.c.elf.cmd}" {compiler.c.elf.flags} -mcpu={build.mcu} "-T{build.variant.path}/{build.ldscript}" "-Wl,-Map,{build.path}/{build.project_name}.map" {compiler.c.elf.extra_flags} -o "{build.path}/{build.project_name}.elf" "-L{build.path}" -lm -lgcc -mthumb -Wl,--cref -Wl,--check-sections -Wl,--gc-sections -Wl,--unresolved-symbols=report-all -Wl,--warn-common -Wl,--warn-section-align -Wl,--warn-unresolved-symbols -Wl,--start-group {object_files} "{build.variant.path}/{build.variant_system_lib}" "{archive_file_path}" -Wl,--end-group
recipe.c.combine.pattern="{compiler.path}{compiler.c.elf.cmd}" {compiler.c.elf.flags} -mcpu={build.mcu} "-T{build.variant.path}/{build.ldscript}" "-Wl,-Map,{build.path}/{build.project_name}.map" {compiler.c.elf.extra_flags} -o "{build.path}/{build.project_name}.elf" "-L{build.path}" -lm -lgcc -mthumb -Wl,--cref -Wl,--check-sections -Wl,--gc-sections -Wl,--unresolved-symbols=report-all -Wl,--warn-common -Wl,--warn-section-align -Wl,--warn-unresolved-symbols -Wl,--start-group {object_files} -Wl,--whole-archive "{archive_file_path}" -Wl,--no-whole-archive -Wl,--end-group

## Create eeprom
recipe.objcopy.eep.pattern=

## Create hex
recipe.objcopy.hex.pattern="{compiler.path}{compiler.elf2hex.cmd}" {compiler.elf2hex.flags} {compiler.elf2hex.extra_flags} "{build.path}/{build.project_name}.elf" "{build.path}/{build.project_name}.bin"

## Compute size
recipe.size.pattern="{compiler.path}{compiler.size.cmd}" -A "{build.path}/{build.project_name}.elf"
recipe.size.regex=^(?:\.text|\.rodata|\.ARM.exidx)\s+([0-9]+).*
recipe.size.regex.data=^(?:\.data|\.bss|\.noinit)\s+([0-9]+).*

## Save Compiled Binary
recipe.output.tmp_file={build.project_name}.bin
recipe.output.save_file={build.project_name}.{build.variant}.bin

# Uploader tools
# -------------------

# Upload using Maple bootloader over DFU
tools.maple_upload.cmd=maple_upload
tools.maple_upload.cmd.windows=maple_upload.bat
tools.maple_upload.path={runtime.hardware.path}/tools/win
tools.maple_upload.path.macosx={runtime.hardware.path}/tools/macosx
tools.maple_upload.path.linux={runtime.hardware.path}/tools/linux
tools.maple_upload.path.linux64={runtime.hardware.path}/tools/linux64
tools.maple_upload.upload.params.verbose=-d
tools.maple_upload.upload.params.quiet=
tools.maple_upload.upload.pattern="{path}/{cmd}" {serial.port.file} {upload.altID} {upload.usbID} "{build.path}/{build.project_name}.bin" {upload.dfuse_addr}

# Generic STM32 upload via serial to Serial Port 1 (pins PA9 and PA10) - note. Boot0 line needs to high on board reset to enable upload via serial
# at the end of the upload the program is automatically run, without the board being reset

# stlink upload
tools.stlink_upload.cmd=stlink_upload
tools.stlink_upload.cmd.windows=stlink_upload.bat
tools.stlink_upload.path.windows={runtime.hardware.path}/tools/win
tools.stlink_upload.path.macosx={runtime.hardware.path}/tools/macosx
tools.stlink_upload.path.linux={runtime.hardware.path}/tools/linux
tools.stlink_upload.path.linux64={runtime.hardware.path}/tools/linux64
tools.stlink_upload.upload.params.verbose=-d
tools.stlink_upload.upload.params.quiet=
tools.stlink_upload.upload.pattern="{path}/{cmd}" {serial.port.file} {upload.altID} {upload.usbID} "{build.path}/{build.project_name}.bin"

# HID upload 2.0 (HID bootloader 2.0 This bootloader will cover the STM32F1 and STM32F4 MCUs)
tools.hid_upload.cmd=hid_upload
tools.hid_upload.cmd.windows=hid-flash.exe
tools.hid_upload.cmd.macosx=hid_flash
tools.hid_upload.path={runtime.hardware.path}/tools/win
tools.hid_upload.path.macosx={runtime.hardware.path}/tools/macosx
tools.hid_upload.path.linux={runtime.hardware.path}/tools/linux
tools.hid_upload.path.linux64={runtime.hardware.path}/tools/linux64
tools.hid_upload.upload.params.verbose=-d
tools.hid_upload.upload.params.quiet=n
tools.hid_upload.upload.pattern="{path}/{cmd}" "{build.path}/{build.project_name}.bin" {serial.port.file}
